Power Amplifier

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

1) 기    능

본 기기는 2U 사이즈에 2,500W/2Ω × 4채널 멀티채널 파워 앰프로 가볍고 컴팩트한 사이즈로 설계되어 Rack 설치 시 적은 공간에 설치가 용이하며, 투어 공연 현장에 최적의 조건을 제공하여야 한다. 특허를 획득한 TD 급 출력단, 앰프의 핵심 기술로서 Class B 설계를 적용한 앰프의 사운드 퀄리티와 Class D설계를 적용한 앰프의 효율성을 하나로 통합한 파워 앰프로, 추가적으로 정류형 스위치 모드 파워 서플라이(R.SMPS)를 사용하여 메인 전압에 유동이 발생하더라도 정확하며 안정적인 출력을 보장하여야 한다. 새롭게 구성되고 보다 업그레이드 된 회로 사용에 R.SMPS 및 TD급 증폭 방식을 사용하여 멀티채널 구동 환경에서도 보다 안정적인 출력을 구동하여야 한다. 특수한 전압 피크 리미터(VPL)을 사용하여 입력 게인을 조정하여야 하고, 채널당 바이어스, VPL을 조정하여 어떠한 부하에서도 최적의 출력을 제공함으로써 하나의 강력한 서브우퍼에서 HF 컴프레션 드라이버 시리즈까지 연결이 가능하여야 한다. 특수한 경고 및 보호회로 시스템을 장착하고 있어서 안전한 출력 회로 및 부하에 상관없이 일정한 동작이 가능하여야 한다.

2) 기기특성

- 정격출력	(2Ω@Ch)	: 4×2,500W

(1㎑)	(4Ω@Ch)	: 4×2,100W

(8Ω@Ch)	: 4×1,300W

(16Ω@Ch)	: 4×660W

(4Ω Bridged)	: 5,000W

(8Ω Bridged)	: 4,200W

(16Ω Bridged)	: 2,600W

- Performance with Gain	: 35㏈ / VPL 150V

- Frequency Response	: 6.8㎐ ~ 34㎑

- THD 20㎐~20㎑ for 1W	: <0.1%

- THD at 1㎑,

1㏈ below clipping	: <0.05%

- S/N Ratio	: >112㏈

- Channel separation

(crosswalk) at 1㎑	: >70㏈

- Input Impedance	: 10㏀

- Common Mode Rejection	: >54㏈, 20㎐ to 20㎑

(CMR)

- Output Impedance @100㎐	: 32mΩ

- Voltage Peak Limiter(VPL)

selectable per Ch	: 150, 121, 101, 83, 70, 56, 46, 38V

- Voltage Peak Limiter(VPL)

Mode	: Hard, Soft

- Amplifier Gain selectable	: 23, 26, 29, 32, 35, 38, 41, 44㏈

- Default Gain	: 35㏈

- Indicator	: Protect / Clip / Signal / Bridge

- Control	: Ch A / Ch B / Ch C / Ch D Volume

Mode / Tone / Matrix Mixer

- Protection	: VHF, DC, High-Impedance,

Low-Impedance, Thermal, PAL, Soft start

- Input Connectors (per Ch)	: 3-Pin XILR, electronically balanced

- Output Connectors (per Ch)	: Binding Posts 2-Pole

- Slew Rate	: 30v/㎲ (Stereo)

- Main Power Supply	: ~230V, 50/60㎐, Fuse : T10A

- Cooling	: 2 Fans, Front to Rear Airflow,

Temperature controlled speed

- Dimensions	: 483(W) × 88(H) × 380(D)㎜

- Weight	: 13㎏

** QD-5+ 및 동등 이상품이어야 한다.